Please review the linked spread sheet

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| |  | | --- | | **JAPANESE** | | **ENGLISH** |  | **Difference** |
| ５９３ | １８１８ |  | ・location of A button 　1818 : lower / 593 : right ・stopwatch mode 　1818 : split time indicator / 593 : lap time indicator |
| ７２９ | ７３０ |  | ・switching between kilograms and pounds 　730 : Available / 729 : Not available |
| ７３３ | ７３４ |  | ・switching between meters and feet ・switching between millibars and inches/Hg 　734 : Available / 733 : Not available |
| ９６０ | ９５０ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between millibars and inches/Hg 　950 : Available / 960 : Not available |
| ９７０ | ９７１ |  | ・switching between meters and feet ・switching between celsius and fahrenheit 　971 : Available / 970 : Not available |
| ９８４ | ９７４ |  | ・switching between celsius and fahrenheit 　974 : Available / 984 : Not available |
| ９８８ | ９８３ |  | ・switching between meters and feet ・switching between millibars and inches/Hg 　983 : Available / 988 : Not available |
| ９９１ | ９６１ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between millibars and inches/Hg 　961 : Available / 991 : Not available |
| ９９７ | ９８７ |  | ・switching between celsius and fahrenheit 　987 : Available / 997 : Not available |
| １１６１ | １１６０ |  | ・switching between meters and feet ・switching between hecto-pascals・milibars and inches/Hg 　1160 : Available / 1161 : Not available |
| １１８４ | １１８３ |  | ・switching between kilograms and pounds 　1183 : Available / 1184 : Not available |
| １２１１ | １２１０ |  | ・switching between celsius and fahrenheit  1210 : Available / 1211 : Not available |
| １２３１ | １２３０ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・milibars and inches/Hg 　1230 : Available / 1231 : Not available |
| １２８３ | １２８２ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・milibars and inches/Hg 　1282 : Available / 1283 : Not available |
| １４０６ | １４０５ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　1405 : Available / 1406 : Not available |
| １４０６ | １５２５ |  | ・Temperature function  1525 : Not available / 1406 : Available  ・switching between meters and feet ・switching between hecto-pascals・milibars and inches/Hg 　1525 : Available / 1406 : Not available |
| １４７３ | １４７２ |  | ・switching between meters and feet ・switching between celsius and fahrenheit  1472 : Available / 1473 : Not available |
| １４９０ | １５５３／１５５４ |  | ・character : KATAKANA(in Japanese)  1553,1554 : Not available / 1490 : Available |
| １５５５ | １５０６/１５０７ |  | ・telephone system setting  1506,1507 : DIGITAL・ANALOGU・DUAL / 1555 : DIGITAL・ANALOG   ・     1506,1507 : Not available / 1555 Available |
| １７０８ | １７５８ |  | ・character : KATAKANA(in Japanese)  1758 : Not available / 1708 : Available  ・Calendar Mode : Rokuyou(in Japanese)  1758 : Not available / 1708 : Available |
| １７２６ | １７５６ |  | ・character : KATAKANA(in Japanese)  1756 : Not available / 1726 : Available  ・Calendar Mode : Rokuyou(in Japanese)  1756 : Not available / 1726 : Available |
| １８８８ | １８８７ |  | ・character : KATAKANA(in Japanese)  1887 : Not available / 1888 : Available |
| １９９９ | １９９８ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　1998 : Available / 1999 : Not available |
| ２０２７ | ２０２６ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　2026 : Available / 2027 : Not available |
| ２０３１ | ２０３０ |  | ・switching between celsius and fahrenheit  2030 : Available / 2031 : Not available |
| ２１４１ | ２１４０ |  | ・Wave Ceptor  2140 : Germany / 2141 : Japan  ・character : KATAKANA(in Japanese)  2140 : Not Available / 2141 : Available |
| ２１７３ | ２１７２ |  | ・switching between meters and feet ・switching between celsius and fahrenheit 　2172 : Available / 2173 : Not available |
| ２１９９ | ２１９８ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　2198 : Available / 2199 : Not available |
| ２２４１ | ２２４０ |  | ・character : KATAKANA(in Japanese)  2240 : Not available / 2241 : Available |
| ２２７２ | ２２７１ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　2271 : Available / 2272 : Not available |
| ２２７４ | ２２７３ |  | ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　2273 : Available / 2274 : Not available |
| ２２９８ | ２２９６ |  | ・Wave Ceptor  2296 : USA / 2298 : Japan |
| ２３０６/２３３４/２３５４/２３５６ | ２３０７/２３３５/２３５５/２３５７ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　2307,2335,2355,2357 : Available / 2306,2334,2354,2356 : Not available |
| ２３４４/２３４８ | ２３４５/２３４７ |  | ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　2345,2347 : Available / 2344,2348 : Not available |
| ２３６３ | ２３６２ |  | ・Wave Ceptor  2362 : Germany / 2363 : Japan  ・character : KATAKANA(in Japanese)  2362 : Not available / 2363 : Available |
| ２３６８ | ２３６７ |  | ・Wave Ceptor  2367 : Germany / 2368 : Japan  ・character : KATAKANA(in Japanese)  2367 : Not available / 2368 : Available |
| ２３７０ | ２３６９ |  | ・Wave Ceptor  2369 : Germany / 2370 : Japan  ・Language Indicator  2369 : Available / 2370 : Not available  ・character : KATAKANA(in Japanese)  2369 : Not available / 2370 : Available |
| ２４１６ | ２４１９ |  | ・character : KATAKANA(in Japanese)  2419 : Not available / 2416 : Available |
| ２４７２ | ２４７１ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals・millibars and inches/Hg 　2471 : Available / 2472 : Not available |
| ２５１１ | ２５１０ |  | ・character : KATAKANA(in Japanese)  2510 : Not available / 2511 : Available |
| ２５３６ | ２５３５ |  | ・switching between centimeters and inches 　2535 : Available / 2536 : Not available  ・switching between kilometers and miles 　2535 : Available / 2536 : Not available |
| ２５７６ | ２５７５ |  | ・switching between centimeters and inches 　2575 : Available / 2576 : Not available  ・switching between kilometers and miles 　2575 : Available / 2576 : Not available |
| ２５８４/２５８８ | ２５８２/２５８６ |  | ・Wave Ceptor  2582・2586 : Germany / 2584・2588 : Japan |
| ２５８４/２５８８ | ２４０６/２５８３/２５８７ |  | ・Wave Ceptor  2406,2583,2587 : USA / 2584・2588 : Japan |
| ２６３１ | ２６３０ |  | ・switching between kilograms and pounds 　2630 : Available / 2631 : Not available  ・switching between centimeters and inches 　2630 : Available / 2631 : Not available  ・switching between kilometers and miles 　2630 : Available / 2631 : Not available |
| ２６９３ | ２６９０ |  | ・Wave Ceptor 　2690 : Not available / 2693 : USA ans Japan |
| ２７４０ | ２７３９ |  | ・Wave Ceptor  2739 : Germany / 2740 : Japan  ・character : KATAKANA(in Japanese)  2739 : Not available / 2740 : Available |
| ２７８１ | ２７８２ |  | the same specification |
| ２８０３ | ２８０２ |  | ・switching between kilograms and pounds 　2802 : Available / 2803 : Not available |
| ２８１５ | ２８１２ |  | ・Wave Ceptor  2812 : Germany / 2815 : USA and Japan |
| ２８２４ | ２８２５ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　2825 : Available / 2824 : Not available |
| ２８７１ | ２８７２ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　2872 : Available / 2871 : Not available |
| ２９７０ | ２９７１ |  | ・Wave Ceptor  2971 : USA / 2970 : USA and Japan |
| ２９７８ | ２９７９ |  | ・switching between kilograms and pounds 　2979 : Available / 2978 : Not available |
| ２９８０ | ２９８１ |  | ・switching between kilograms and pounds 　2981 : Available / 2980 : Not available |
| ２９９７ | ３０１６/３０１７ |  | ・Wave Ceptor  3016 : USA /3017 : Germany and UK / 2997 : USA and Japan |
| ３０１２ | ３０２４ |  | ・Wave Ceptor  3024 : USA / 3012 : USA and Japan |
| ３０１３ | ３０１４ |  | ・switching between kilograms and pounds 　3014 : Available / 3013 : Not available  ・switching between grams and ounces 　3014 : Available / 3013 : Not available |
| ３０２１ | ３０２２ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　3022 : Available / 3021 : Not available |
| ３０４２ | ３０４３ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　3043 : Available / 3042 : Not available |
| ３０６４ | ３０６８ |  | ・Wave Ceptor  3068 : non / 3064 : USA and Japan  ・switching between celsius and fahrenheit 　3068 : Available / 3064 : Not available |
| ３０９８ | ３０９９ |  | ・switching between kilograms and pounds 　3099 : Available / 3098 : Not available  ・switching between centimeters and inches 　3099 : Available / 3098 : Not available |
| ３１０２ | ２８９４ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　2894 : Available / 3102 : Not available |
| ３１４１ | ３１４３ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　3143 : Available / 3141 : Not available |
| ３１４１ | ３１４４ |  | ・Wave Ceptor  3144 : non / 3141 : USA, UK, Germany and Janapn  ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg  3144 : Available / 3141 Not available |
| ３１５６ | ３１５７ |  | ・switching between celsius and fahrenheit 　3157 : Available / 3156 : Not available |
| ３２０３ | ３２０５/３２０６ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　3205,3206 : Available / 3203 : Not available |
| ３２０７ | ３０７１ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　3071 : Available / 3207 : Not available |
| ３２９２ | ３２８３ |  | ・switching between centimeters and inches 　3283 : Available / 3292 : Not available  ・switching between kilometers and miles 　3283 : Available / 3292 : Not available |
| ３３１５ | ３３１２ |  | ・Wave Ceptor  3312 : Germany / 3315 : Japan |
| ３３３０ | ３３３３ |  | ・Wave Ceptor  3333 : non / 3330 : USA and Japan |
| ３７３１ | ３７３３/３７３４ |  | ・Wave Ceptor  3733・3734 : Germany and UK / 3731 : Japan |
| ３７４６ | ３７４７/３７４８/３７４９ |  | ・Wave Ceptor  3747 : USA / 3748,3749 : Germany and UK / 3746 : USA and Japan |
| ３７５３ | ３３２９ |  | the same specification |
| ３７６６ | ３７７２/３７８６ |  | ・Wave Ceptor  3772 : USA / 3786 : non / 3766 : USA and Japan |
| ４３０２ | ３７３２ |  | ・Wave Ceptor  3732 : USA and Japan / 4302 : Japan |
| ４３１５ | ４３１６/４３１７/４３１８ |  | ・Wave Ceptor  4316 : USA / 4317,4318 : Germany and UK / 4315 : Japan  ・GMT Differential Value(when set the time) 　4316,4317,4318 : Available / 4315 : Not available |
| ４３４９ | ４３５０/４３６４ |  | ・Home Time Zone 　4350,4364->4349 : ET->NYC, CT->CHI, MT->DEN, PT->LAX, -9->non, -10->non |
| ４３８２ | ４３８３/４３８４ |  | ・Wave Ceptor  4383 : USA / 4384 : Germany and UK / 4382 : Japan  ・GMT Differential Value(when set the time) 　4383,4384 : Available / 4382 : Not available |
| ４７０７ | ４３３５/４３４８ |  | ・switching between celsius and fahrenheit 　4335,4348 : Available / 4707 : Not available |
| ４７０７ | ４７７９/４７８０/５０２７ |  | ・Mute function  4779,4780,5027 : Non / 4707 : Available  ・the number of button  4779,4780,5027 : 4 buttons / 4707 : 5 buttons("B" button is Illumination function only.)  ・switching between celsius and fahrenheit 　4779,4780,5027 : Available / 4707 : Not available |
| ４７２７ | ４３２９ |  | the same specification |
| ４７３０ | ４３３４/４７３８ |  | ・switching between celsius and fahrenheit 　4334,4738 : Available / 4730 : Not available |
| ４７７１ | ４７７２/４７７３/４７７４ |  | ・Wave Ceptor  4772 : USA / 4773,4774 : Germany and UK / 4771 : USA and Japan |
| ５１１０ | ５０６４ |  | ・the small circle at 3 o'clock on the display  5064 : with / 5110 : without |
| ５１２０ | ４７３２/４７３３/５０５６ |  | ・switching between celsius and fahrenheit 　4732,4733,5056 : Available / 5120 : Not available |
| ５１３３ | ５１４５ |  | ・Battery level hand 　5145 : Available / 5133 : Not available |
| ５１９５ | ５１９６/５２５２/５３０１ |  | ・location of Day Indicator 　5196 : at 4 o'clock / 5195 : at 5 o'clock  ・number of characters showing in the window of Day Indicator 　5196 : 3 caracters / 5195 : 1 caracter |
| ５２４１ | ５２４２ |  | ・switching between meters and feet ・switching between celsius and fahrenheit ・switching between hecto-pascals and inches/Hg 　5242 : Available / 5241 : Not available |
| ５２５３ | ５１９６/５２５２/５３０１ |  | ・function which automatically detect and adjust the position of the second hand as adjusting the home position 　5196,5252,5301 : Available / 5253 : Not available |
|  |  |  |  |