**CS-55P Discontinued Keyboard Stand (screw dimensions)**

The dimensions of the screws are as follows.

screw B: M5X40mm, pan head double sems screw

screw F: M6X30mm, joint-connector　JB-A

screw G: M6X55mm, joint-connector　JB-A

screw H: M6X16mm, joint-connector